**SPECIFICATION SHEET:**



**CP Furniture - Cambio**

**FULL LENGTH LOCKERS**

**Dimensions:**

**Height Width Depth Nesting**

1850 mm 300 mm 525 mm 1 2 3 4

1850 mm 400 mm 525 mm 1 2 3

Single Tier/2/3/4/5/6/Z locker

**Strength and Security with Style**

Carcass Durable Sheet Steel construction with multi-functional step system and overlapping doors

Ventilation system with the SVL concept as standard

Double Walled for high stability

Body and steel doors zinc plated as a standard

Perforated hat shelf to improve ventilation

Doors 13mm Compact Grade Laminate Fundermax or Formica

End Panels 13mm Compact Grade Laminate Fundermax or Formica if required

Hinges Stainless Steel Concealed Hinges

Door opening limiter of 90 degrees and doorstop silencers as standard

Accessories Sturdy Wardrobe Rail made of oval profile with 4 twist proof hooks and

Wide Variety of internal fittings

Benches available in various designs/finishes

Base Height Adjustable with feet 150mm – 190mm easily adjustable from inside or outside locker

Plastic feet or Steel Plinth as standard.

Reconfiguration Internal make up of locker can be changed eg a 2 Tier can become a 3 tier with one new door and shelf if more lockers are required in the future

Colours There are standard paint and laminate colours in stock but products can be made to specification for project work.

Nesting: Lockers can be supplied as single units or nested in groups during the manufacturing process.

All lockers are holed in back and sides to enable them to be bolted together into rows or back

to back to suit your requirements. **Note:** When preparing locker room layouts allow

approximately 4 mm extra for each nest for rivet heads at the sides of lockers in each row.

Locking: Cam lock or Pad Lock as standard.

Digilocks, RFID, fingerprint, eye retina recognition, online and off line systems etc all available at an up charge to Cam or Pad lock price

**OPTIONAL EXTRAS:** The following can be supplied at an additional cost and, if included, will be specified in the

quotation.

Locker Numbering:

a) Number Label

b) Number Plate

c) Number Discs

d) Etched Numbers into laminate

Stands/with Seats: Lockers can be provided with either stands or stands with seats with or without adjustable feet.

Sloping Tops: Lockers can be manufactured with a sloping top. Gradient 1:3

Integrated Power/USB port

**Extras**

**Drawings:** Allied offer full autocad services for projects and will create layouts and 3d Renders for your project once given the brief for same.

**Installation:** Allied offers a full installation service for its products.

**Bespoke:** We have the ability to customise our products to meet your requirement and space, providing solutions for awkward corners, uneven floors or even curved walls.

**After-sales Service:** All of our products are supported by the Allied Service team who provide technical advice, maintenance schemes, prompt delivery of replacement keys/parts and product refurbishment.

**Allied Workspace**

24 Tolka Valley Business Park, Glasnevin, Dublin 11

+353 1 8532222

For assistance with specification please contact **Jane Delany**

janedelany@allied.ie

+353 86 8116052

|  |  |
| --- | --- |
|  | Height adjustable feetHeight adjustable feet from 150 to 190 mm, can be adjusted from the inside and outside. |
|  | Door opening limiter 90° (standard design). |
|  | Damp-proofInsulation of the door sealed on all sides =100% damp-proof. |
|  | Labeling and orientation:through individual numbering and pictograms. |
| http://nwc-ambienta.com/images/ambientasecure/digilock_rfid.png | For integration with Cambio:Digilock’s RFID lock system will work with the students building cards  |